Hide navigation sidebar
Hide table of contents sidebar
Skip to content
Back to top
View this page
Toggle table of contents sidebar

# PyStim Configuration

This class provides a set of methods to control PyStim configuration.

## Exception printing control

- enable_exception_printing() – Enables printing of Python exceptions to the HDL simulator console. Use this method to turn on detailed debugging output when a Python error occurs.

- disable_exception_printing() – Disables printing of Python exceptions to the console. Useful if exception output is not needed or is obscuring other messages.

## Simulation flow control on exception

- stop_on_exception() – Configures the simulator to halt execution when a Python exception occurs. Recommended for catching critical errors that should terminate the simulation.

- continue_on_exception() – Configures the simulator to continue execution despite encountering a Python exception. This can be used to allow the simulation to proceed when exceptions are non-critical.